S504 Title: **Extrication Hydraulic Pump - 1481**

**Start**

1. Check gas, hydraulic oil, engine oil
2. Connect hose(s)
3. Fuel cap vent to ON
4. Engine switch to ON
5. Choke to CHOKE. To RUN when warm
6. Ecothrottle to full speed
7. Pull starter cord

**Stop**

1. Engine switch to OFF. Leave off for storage
2. Choke to CHOKE
3. Fuel cap vent to OFF once engine cool.

Leave OFF for storage