S512 **Hose Care and Testing**

**Procedures:**

1. After each use, hose will be:
2. Inspected for breaks and/or holes
3. Cleaned by washing with soap and water if necessary
4. Drain thoroughly and reloaded or placed in storage
5. Canvas jacketed hose should be dried prior to storage and placed on top of newer hose in hose bed
6. All couplings shall be checked, washed and lubricated as needed
7. Hose will be inspected and tested every three (3) years