S502 **Station Generator**

**Procedures:**

* All Station Emergency Generators are on an annual maintenance program with a third-party provider.
* Regular PM procedures will include physical inspections for obstructions, overall condition and indicator status lights. Personnel will report all status light conditions other than GREEN to the Station Captain.